Driver package for CUSTOM ENGINEERING VKP112 printer model

OS Supported:

Windows XP   		
Windows Vista 	x86 (User Account Control disabled)
Windows Vista 	x64 (User Account Control disabled)
Windows 7 	x86 (User Account Control disabled)
Windows 7 	x64 (User Account Control disabled)

Installation procedure:

Serial and parallel interface
For (W2K, XP, W2K3, Vista, 7) you must execute the standard printer installation procedure.

USB interface
Follow the automatic wizard procedure.

This driver supports one model of printer:
"CUSTOM VKP112"

The "CUSTOM VKP112" can prints on a paper width size of 112mm.

The "CUSTOM VKP112" printer supports some page format:

"VKP112 Roll"
"VKP112 Roll+"
"VKP112 Roll++"
"VKP112 115mm"
"VKP112 230mm"
"VKP112 340mm"
"VKP112 450mm"

[ the defalut installation page is "VKP112 Roll" ]

If the system driver properties section shows these format pages and other not here
specified, you must select only the above mentioned pages format.

